{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":5,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["NO.","类别","需求","示意图","状态"]
[{"$f":"ROW()-1","v":1},"新增","EAP监控看板增加每条线体的稼动率",null,"ongoing"]
[{"$f":"ROW()-1","v":2},"优化","EAP监控看板选择某一个机种后，仪表盘稼动率刷新不出来（刷新时间过长）",null,"ongoing"]
[3,"优化","EAP监控看板显示时AA放到LHA下边，以各楼层间，先COB再EOL，COB中先DA&WB线体，线体完后再LHA，最后AA，按照工序排序",null,"ongoing"]
[4,"新增","监控看板对试产的所有设备不计算到稼动率中",null,"ongoing"]
[5,"新增","在EAP看板这里增加日期选项，在选择日期后，可以通过选择班别来选择白班/夜班，选择白班就是8:30-20:30这段时间的设备稼动率，设备状态以20:30时的状态显示，夜班同理，选择一整天就按照8:30-8:30  24H来核算稼动率，状态以最终24H时的状态显示，班别未选择时，默认选择一整天进行显示，",null,"ongoing"]
[6,"优化","仪表盘稼动率与所选设备稼动率不一致",null,"ongoing"]
[7,"新增","EAP监控看板上增加时钟，实时显示北京时间",null,"ongoing"]